[ Main Table Of Contents | Table Of Contents | Keyword Index | Categories | Modules | Applications ]

# units(n) 1.2 tcllib "Convert and manipulate quantities with units"

## Name

units - unit conversion

## Synopsis

- package require Tcl 8.1
- package require units ?2.1?

- ::units::convert value targetUnits
- ::units::reduce unitString
- ::units::new name baseUnits

## Description

This library provides a conversion facility from a variety of scientific and engineering shorthand notations into floating point numbers. This allows application developers to easily convert values with different units into uniformly scaled numbers.

The units conversion facility is also able to convert between compatible units. If, for example, a application is expecting a value in ohms (Resistance), and the user specifies units of milliwebers/femtocoulomb, the conversion routine will handle it appropriately. An error will be generated if an incorrect conversion is attempted.

Values are scaled from one set of units to another by dimensional analysis. Both the value units and the target units are reduced into primitive units and a scale factor. Units are checked for compatibility, and the scale factors are applied by multiplication and division. This technique is extremely flexible and quite robust.

New units and new unit abbreviations can be defined in terms of existing units and abbreviations. It is also possible to define a new primitive unit, although that will probably be unnecessary. New units will most commonly be defined to accommodate non-SI measurement systems, such as defining the unit inch as 2.54 cm.

## COMMANDS

::units::convert value targetUnits

  Converts the value string into a floating point number, scaled to the specified targetUnits. The value string may contain a number and units. If units are specified, then they must be compatible with the targetUnits. If units are not specified for the value, then it will be scaled to the target units. For example,

      % ::units::convert "2.3 miles" km
      3.7014912
      % ::units::convert 300m/s miles/hour
      671.080887616
      % ::units::convert "1.0 m kg/s^2" newton
      1.0
      % ::units::convert 1.0 millimeter
      1000.0

::units::reduce unitString

  Returns a unit string consisting of a scale factor followed by a space separated list of sorted and reduced primitive units. The reduced unit string may include a forward-slash (separated from the surrounding primitive subunits by spaces) indicating that the remaining subunits are in the denominator. Generates an error if the unitString is invalid.

      % ::units::reduce pascal
      1000.0 gram / meter second second

::units::new name baseUnits

  Creates a new unit conversion with the specified name. The new unit name must be only alphabetic (upper or lower case) letters. The baseUnits string can consist of any valid units conversion string, including constant factors, numerator and denominator parts, units with prefixes, and exponents. The baseUnits may contain any number of subunits, but it must reduce to primitive units. BaseUnits could also be the string -primitive to represent a new kind of quantity which cannot be derived from other units. But you probably would not do that unless you have discovered some kind of new universal property.

      % ::units::new furlong "220 yards"
      % ::units::new fortnight "14 days"
      % ::units::convert 100m/s furlongs/fortnight
      601288.475303

## UNIT STRING FORMAT

Value and unit string format is quite flexible. It is possible to define virtually any combination of units, prefixes, and powers. Valid unit strings must conform to these rules.

- A unit string consists of an optional scale factor followed by zero or more subunits. The scale factor must be a valid floating point number, and may or may not be separated from the subunits. The scale factor could be negative.

- Subunits are separated form each other by one or more separator characters, which are space (" "), hyphen ("-"), asterisk ("*"), and forward-slash ("/"). Sure, go ahead and complain about using a minus sign ("-") to represent multiplication. It just isn't sound mathematics, and, by rights, we should require everyone to use the asterisk ("*") to separate all units. But the bottom line is that complex unit strings like m-kg/s^2 are pleasantly readable.

- The forward-slash seperator ("/") indicates that following subunits are in the denominator. There can be at most one forward-slash separator.

- Subunits can be floating point scale factors, but with the exception of the leading scale factor, they must be surrounded by valid separators. Subunit scale factors cannot be negative. (Remember that the hyphen is a unit separator.)

- Subunits can be valid units or abbreviations. They may include a prefix. They may include a plural suffix "s" or "es". They may also include a power string denoted by a circumflex ("^"), followed by a integer, after the unit name (or plural suffix, if there is one). Negative exponents are not allowed. (Remember that the hyphen is a unit separator.)

### Example Valid Unit Strings

    Unit String              Reduced Unit String
    ------------------------------------------------------------
    meter                    1.0 meter
    kilometer                1000.0 meter
    km                       1000.0 meter
    km/s                     1000.0 meter / second
    /microsecond             1000000.0 / second
    /us                      1000000.0 / second
    kg-m/s^2                 1000.0 gram meter / second second
    30second                 30.0 second
    30 second                30.0 second
    30 seconds               30.0 second
    200*meter/20.5*second    9.75609756098 meter / second

## SI UNITS

The standard SI units are predefined according to NIST Special Publication 330. Standard units for both SI Base Units (Table 1) and SI Derived Units with Special Names (Tables 3a and 3b) are included here for reference. Each standard unit name and abbreviation are included in this package.

### SI Base Units

    Quantity                Unit Name    Abbr.
    ---------------------------------------------
    Length                  meter        m
    Mass                    kilogram     kg
    Time                    second       s
    Current                 ampere       A
    Temperature             kelvin       K
    Amount                  mole         mol
    Luminous Intensity      candela      cd

### SI Derived Units with Special Names

    Quantity                Unit Name    Abbr.   Units     Base Units
    --------------------------------------------------------------------
    plane angle             radian      rad     m/m       m/m
    solid angle             steradian   sr      m^2/m^2   m^2/m^2
    frequency               hertz       Hz                /s
    force                   newton      N                 m-kg/s^2
    pressure                pascal      Pa      N/m^2     kg/m-s^2
    energy, work            joule       J       N-m       m^2-kg/s^2
    power, radiant flux     watt        W       J/s       m^2-kg/s^3
    electric charge         coulomb     C                 s-A
    electric potential      volt        V       W/A       m^2-kg/s^3-A
    capacitance             farad       F       C/V       s^4-A^2/m^2-kg
    electric resistance     ohm                 V/A       m^2-kg/s^3-A^2
    electric conductance    siemens     S       A/V       s^3-A^2/m^2-kg
    magnetic flux           weber       Wb      V-s       m^2-kg/s^2-A
    magnetic flux density   tesla       T       Wb/m^2    kg/s^2-A
    inductance              henry       H       Wb/A      m^2-kg/s^2-A^2
    luminous flux           lumen       lm                cd-sr
    illuminance             lux         lx      lm/m^2    cd-sr/m^2
    activity (of a
    radionuclide)           becquerel   Bq                /s
    absorbed dose           gray        Gy      J/kg      m^2/s^2
    dose equivalent         sievert     Sv      J/kg      m^2/s^2

Note that the SI unit kilograms is actually implemented as grams because 1e-6 kilogram = 1 milligram, not 1 microkilogram. The abbreviation for Electric Resistance (ohms), which is the omega character, is not supported.

Also note that there is no support for Celsius or Farenheit temperature. The units conversion routines can only scale values with multiplication and division, so it is not possible to convert from thermodynamic temperature (kelvins) to absolute degrees Celsius or Farenheit. Conversion of thermodynamic quantities, such as thermal expansion (per unit temperature), however, are easy to add to the units library.

SI Units can have a multiple or sub-multiple prefix. The prefix or its abbreviation should appear before the unit, without spaces. Compound prefixes are not allowed, and a prefix should never be used alone. These prefixes are defined in Table 5 of Special Publication 330.

### SI Prefixes

    Prefix Name     Abbr.   Factor
    ---------------------------------------
    yotta           Y       1e24
    zetta           Z       1e21
    exa             E       1e18
    peta            P       1e15
    tera            T       1e12
    giga            G       1e9
    mega            M       1e6
    kilo            k       1e3
    hecto           h       1e2
    deka            da      1e1
    deca                    1e1
    deci            d       1e-1
    centi           c       1e-2
    milli           m       1e-3
    micro           u       1e-6
    nano            n       1e-9
    pico            p       1e-12
    femto           f       1e-15
    atto            a       1e-18
    zepto           z       1e-21
    yocto           y       1e-24

Note that we define the same prefix with both the USA ("deka") and non-USA ("deca") spellings. Also note that we take the liberty of allowing "micro" to be typed as a "u" instead of the Greek character mu.

Many non-SI units are commonly used in applications. Appendix B.8 of NIST Special Publication 811 lists many non-SI conversion factors. It is not possible to include all possible unit definitions in this package. In some cases, many different conversion factors exist for a given unit, depending on the context. (The appendix lists over 40 conversions for British thermal units!) Application specific conversions can always be added using the new command, but some well known and often used conversions are included in this package.

### Non-SI Units

    Unit Name            Abbr.    Base Units
    --------------------------------------------------
    angstrom                      1.0E-10 m
    astronomicalUnit     AU       1.495979E11 m
    atmosphere                    1.01325E5 Pa
    bar                           1.0E5 Pa
    calorie                       4.1868 J
    curie                         3.7E10 Bq
    day                           8.64E4 s
    degree                        1.745329E-2 rad
    erg                           1.0E-7 J
    faraday                       9.648531 C
    fermi                         1.0E-15 m
    foot                 ft       3.048E-1 m
    gauss                         1.0E-4 T
    gilbert                       7.957747E-1 A
    grain                gr       6.479891E-5 kg
    hectare              ha       1.0E4 m^2
    hour                 h        3.6E3 s
    inch                 in       2.54E-2 m
    lightYear                     9.46073E15 m
    liter                L        1.0E-3 m^3
    maxwell              Mx       1.0E-8 Wb
    mho                           1.0 S
    micron                        1.0E-6 m
    mil                           2.54E-5 m
    mile                 mi       1.609344E3 m
    minute               min      6.0E1 s
    parsec               pc       3.085E16 m
    pica                          4.233333E-3 m
    pound                lb       4.535924E-1 kg
    revolution                    6.283185 rad
    revolutionPerMinute  rpm      1.047198E-1 rad/s
    yard                 yd       9.144E-1 m
    year                          3.1536E7 s

### Quantities and Derived Units with Special Names

This units conversion package is limited specifically to unit reduction, comparison, and scaling. This package does not consider any of the quantity names for either base or derived units. A similar implementation or an extension in a typed or object-oriented language might introduce user defined types for the quantities. Quantity type checking could be used, for example, to ensure that all length values properly reduced to meters, or that all velocity values properly reduced to meters/second.

A C implementation of this package has been created to work in conjunction with the Simplified Wrapper Interface Generator (http://www.swig.org/). That package (units.i) exploits SWIG's typemap system to automatically convert script quantity strings into floating point quantities. Function arguments are specified as quantity types (e.g., typedef float Length), and target units (expected by the C application code) are specified in an associative array. Default units are also defined for each quantity type, and are applied to any unit-less quantity strings.

A units system enhanced with quantity type checking might benefit from inclusion of other derived types which are expressed in terms of special units, as illustrated in Table 2 of NIST Publication 330. The quantity area, for example, could be defined as units properly reducing to meter^2, although the utility of defining a unit named square meter is arguable.

## REFERENCES

The unit names, abbreviations, and conversion values are derived from those published by the United States Department of Commerce Technology Administration, National Institute of Standards and Technology (NIST) in NIST Special Publication 330: The International System of Units (SI) and NIST Special Publication 811: Guide for the Use of the International System of Units (SI). Both of these publications are available (as of December 2000) from http://physics.nist.gov/cuu/Reference/contents.html

The ideas behind implementation of this package is based in part on code written in 1993 by Adrian Mariano which performed dimensional analysis of unit strings using fixed size tables of C structs. After going missing in the late 1990's, Adrian's code has reappeared in the GNU Units program at http://www.gnu.org/software/units/

## AUTHORS

Robert W. Techentin

## Bugs, Ideas, Feedback

This document, and the package it describes, will undoubtedly contain bugs and other problems. Please report such in the category units of the Tcllib Trackers. Please also report any ideas for enhancements you may have for either package and/or documentation.

## Keywords

angle, constants, conversion, distance, radians, unit

## Copyright

Copyright © 2000-2005 Mayo Foundation